P: /devices/pci0000:00/0000:00:08.1/0000:05:00.4/usb3/3-2
N: bus/usb/003/004=12011001000000087E14162002000102000109022700010100A0320904000003FF000000070581024000000705020240000007058303040014
E: BUSNUM=003
E: CURRENT_TAGS=:seat:
E: DEVNAME=/dev/bus/usb/003/004
E: DEVNUM=004
E: DEVTYPE=usb_device
E: DRIVER=usb
E: ID_AUTOSUSPEND=1
E: ID_BUS=usb
E: ID_FOR_SEAT=usb-pci-0000_05_00_4-usb-0_2
E: ID_MODEL=Biometric_Coprocessor
E: ID_MODEL_ENC=Biometric\x20Coprocessor
E: ID_MODEL_FROM_DATABASE=Biometric Touchchip/Touchstrip Fingerprint Sensor
E: ID_MODEL_ID=2016
E: ID_PATH=pci-0000:05:00.4-usb-0:2
E: ID_PATH_TAG=pci-0000_05_00_4-usb-0_2
E: ID_PERSIST=0
E: ID_REVISION=0002
E: ID_SERIAL=UPEK_Biometric_Coprocessor
E: ID_USB_INTERFACES=:ff0000:
E: ID_VENDOR=UPEK
E: ID_VENDOR_ENC=UPEK
E: ID_VENDOR_FROM_DATABASE=Upek
E: ID_VENDOR_ID=147e
E: MAJOR=189
E: MINOR=259
E: PRODUCT=147e/2016/2
E: SUBSYSTEM=usb
E: TAGS=:seat:
E: TYPE=0/0/0
A: authorized=1\n
A: avoid_reset_quirk=0\n
A: bConfigurationValue=1\n
A: bDeviceClass=00\n
A: bDeviceProtocol=00\n
A: bDeviceSubClass=00\n
A: bMaxPacketSize0=8\n
A: bMaxPower=100mA\n
A: bNumConfigurations=1\n
A: bNumInterfaces= 1\n
A: bcdDevice=0002\n
A: bmAttributes=a0\n
A: busnum=3\n
A: configuration=
H: descriptors=12011001000000087E14162002000102000109022700010100A0320904000003FF000000070581024000000705020240000007058303040014
A: dev=189:259\n
A: devnum=4\n
A: devpath=2\n
L: driver=../../../../../../bus/usb/drivers/usb
L: firmware_node=../../../../../LNXSYSTM:00/LNXSYBUS:00/PNP0A08:00/device:10/device:1f/device:20/device:22
A: idProduct=2016\n
A: idVendor=147e\n
A: ltm_capable=no\n
A: manufacturer=UPEK\n
A: maxchild=0\n
A: physical_location/dock=no\n
A: physical_location/horizontal_position=left\n
A: physical_location/lid=no\n
A: physical_location/panel=top\n
A: physical_location/vertical_position=upper\n
L: port=../3-0:1.0/usb3-port2
A: power/active_duration=76426\n
A: power/autosuspend=2\n
A: power/autosuspend_delay_ms=2000\n
A: power/connected_duration=5956377\n
A: power/control=auto\n
A: power/level=auto\n
A: power/persist=0\n
A: power/runtime_active_time=77623\n
A: power/runtime_status=active\n
A: power/runtime_suspended_time=5878510\n
A: power/wakeup=disabled\n
A: power/wakeup_abort_count=\n
A: power/wakeup_active=\n
A: power/wakeup_active_count=\n
A: power/wakeup_count=\n
A: power/wakeup_expire_count=\n
A: power/wakeup_last_time_ms=\n
A: power/wakeup_max_time_ms=\n
A: power/wakeup_total_time_ms=\n
A: product=Biometric Coprocessor\n
A: quirks=0x0\n
A: removable=removable\n
A: rx_lanes=1\n
A: speed=12\n
A: tx_lanes=1\n
A: urbnum=1200\n
A: version= 1.10\n

P: /devices/pci0000:00/0000:00:08.1/0000:05:00.4/usb3
N: bus/usb/003/001=12010002090001406B1D020019050302010109021900010100E0000904000001090000000705810304000C
E: BUSNUM=003
E: CURRENT_TAGS=:seat:
E: DEVNAME=/dev/bus/usb/003/001
E: DEVNUM=001
E: DEVTYPE=usb_device
E: DRIVER=usb
E: ID_AUTOSUSPEND=1
E: ID_BUS=usb
E: ID_FOR_SEAT=usb-pci-0000_05_00_4
E: ID_MODEL=xHCI_Host_Controller
E: ID_MODEL_ENC=xHCI\x20Host\x20Controller
E: ID_MODEL_FROM_DATABASE=2.0 root hub
E: ID_MODEL_ID=0002
E: ID_PATH=pci-0000:05:00.4
E: ID_PATH_TAG=pci-0000_05_00_4
E: ID_REVISION=0519
E: ID_SERIAL=Linux_5.19.14-200.fc36.x86_64_xhci-hcd_xHCI_Host_Controller_0000:05:00.4
E: ID_SERIAL_SHORT=0000:05:00.4
E: ID_USB_INTERFACES=:090000:
E: ID_VENDOR=Linux_5.19.14-200.fc36.x86_64_xhci-hcd
E: ID_VENDOR_ENC=Linux\x205.19.14-200.fc36.x86_64\x20xhci-hcd
E: ID_VENDOR_FROM_DATABASE=Linux Foundation
E: ID_VENDOR_ID=1d6b
E: MAJOR=189
E: MINOR=256
E: PRODUCT=1d6b/2/519
E: SUBSYSTEM=usb
E: TAGS=:seat:
E: TYPE=9/0/1
A: authorized=1\n
A: authorized_default=1\n
A: avoid_reset_quirk=0\n
A: bConfigurationValue=1\n
A: bDeviceClass=09\n
A: bDeviceProtocol=01\n
A: bDeviceSubClass=00\n
A: bMaxPacketSize0=64\n
A: bMaxPower=0mA\n
A: bNumConfigurations=1\n
A: bNumInterfaces= 1\n
A: bcdDevice=0519\n
A: bmAttributes=e0\n
A: busnum=3\n
A: configuration=
H: descriptors=12010002090001406B1D020019050302010109021900010100E0000904000001090000000705810304000C
A: dev=189:256\n
A: devnum=1\n
A: devpath=0\n
L: driver=../../../../../bus/usb/drivers/usb
L: firmware_node=../../../../LNXSYSTM:00/LNXSYBUS:00/PNP0A08:00/device:10/device:1f/device:20
A: idProduct=0002\n
A: idVendor=1d6b\n
A: interface_authorized_default=1\n
A: ltm_capable=no\n
A: manufacturer=Linux 5.19.14-200.fc36.x86_64 xhci-hcd\n
A: maxchild=4\n
A: power/active_duration=95134\n
A: power/autosuspend=0\n
A: power/autosuspend_delay_ms=0\n
A: power/connected_duration=6808009\n
A: power/control=auto\n
A: power/level=auto\n
A: power/runtime_active_time=95126\n
A: power/runtime_status=active\n
A: power/runtime_suspended_time=6712879\n
A: power/wakeup=disabled\n
A: power/wakeup_abort_count=\n
A: power/wakeup_active=\n
A: power/wakeup_active_count=\n
A: power/wakeup_count=\n
A: power/wakeup_expire_count=\n
A: power/wakeup_last_time_ms=\n
A: power/wakeup_max_time_ms=\n
A: power/wakeup_total_time_ms=\n
A: product=xHCI Host Controller\n
A: quirks=0x0\n
A: removable=unknown\n
A: rx_lanes=1\n
A: serial=0000:05:00.4\n
A: speed=480\n
A: tx_lanes=1\n
A: urbnum=441\n
A: version= 2.00\n

P: /devices/pci0000:00/0000:00:08.1/0000:05:00.4
E: DRIVER=xhci_hcd
E: ID_MODEL_FROM_DATABASE=Renoir/Cezanne USB 3.1
E: ID_PCI_CLASS_FROM_DATABASE=Serial bus controller
E: ID_PCI_INTERFACE_FROM_DATABASE=XHCI
E: ID_PCI_SUBCLASS_FROM_DATABASE=USB controller
E: ID_VENDOR_FROM_DATABASE=Advanced Micro Devices, Inc. [AMD]
E: MODALIAS=pci:v00001022d00001639sv00001043sd0000201Fbc0Csc03i30
E: PCI_CLASS=C0330
E: PCI_ID=1022:1639
E: PCI_SLOT_NAME=0000:05:00.4
E: PCI_SUBSYS_ID=1043:201F
E: SUBSYSTEM=pci
A: ari_enabled=0\n
A: broken_parity_status=0\n
A: class=0x0c0330\n
H: [encoded data, 8199 characters]
A: consistent_dma_mask_bits=64\n
A: current_link_speed=16.0 GT/s PCIe\n
A: current_link_width=16\n
A: d3cold_allowed=1\n
A: dbc=disabled\n
A: device=0x1639\n
A: dma_mask_bits=64\n
L: driver=../../../../bus/pci/drivers/xhci_hcd
A: driver_override=(null)\n
A: enable=1\n
L: firmware_node=../../../LNXSYSTM:00/LNXSYBUS:00/PNP0A08:00/device:10/device:1f
L: iommu=../../0000:00:00.2/iommu/ivhd0
L: iommu_group=../../../../kernel/iommu_groups/6
A: irq=45\n
A: link/l0s_aspm=0\n
A: link/l1_aspm=0\n
A: local_cpulist=0-15\n
A: local_cpus=ffff\n
A: max_link_speed=16.0 GT/s PCIe\n
A: max_link_width=16\n
A: modalias=pci:v00001022d00001639sv00001043sd0000201Fbc0Csc03i30\n
A: msi_bus=1\n
A: msi_irqs/46=msix\n
A: msi_irqs/47=msix\n
A: msi_irqs/48=msix\n
A: msi_irqs/49=msix\n
A: msi_irqs/50=msix\n
A: msi_irqs/51=msix\n
A: msi_irqs/52=msix\n
A: msi_irqs/53=msix\n
A: numa_node=-1\n
A: pools=poolinfo - 0.1\nbuffer-2048         0    0 2048  0\nbuffer-512          0    0  512  0\nbuffer-128          0    0  128  0\nbuffer-32           0    0   32  0\nxHCI 1KB stream ctx arrays    0    0 1024  0\nxHCI 256 byte stream ctx arrays    0    0  256  0\nxHCI input/output contexts    4    5 2112  5\nxHCI ring segments   22   26 4096 26\nbuffer-2048         0    0 2048  0\nbuffer-512          0    0  512  0\nbuffer-128          0    0  128  0\nbuffer-32           0    0   32  0\n
A: power/control=on\n
A: power/runtime_active_time=6808494\n
A: power/runtime_status=active\n
A: power/runtime_suspended_time=0\n
A: power/wakeup=enabled\n
A: power/wakeup_abort_count=0\n
A: power/wakeup_active=0\n
A: power/wakeup_active_count=0\n
A: power/wakeup_count=0\n
A: power/wakeup_expire_count=0\n
A: power/wakeup_last_time_ms=0\n
A: power/wakeup_max_time_ms=0\n
A: power/wakeup_total_time_ms=0\n
A: power_state=D0\n
A: reset_method=pm\n
A: resource=0x00000000fc200000 0x00000000fc2fffff 0x0000000000140204\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n
A: revision=0x00\n
A: subsystem_device=0x201f\n
A: subsystem_vendor=0x1043\n
A: vendor=0x1022\n

P: /devices/pci0000:00/0000:00:08.1
E: DRIVER=pcieport
E: ID_MODEL_FROM_DATABASE=Renoir Internal PCIe GPP Bridge to Bus
E: ID_PCI_CLASS_FROM_DATABASE=Bridge
E: ID_PCI_INTERFACE_FROM_DATABASE=Normal decode
E: ID_PCI_SUBCLASS_FROM_DATABASE=PCI bridge
E: ID_VENDOR_FROM_DATABASE=Advanced Micro Devices, Inc. [AMD]
E: MODALIAS=pci:v00001022d00001635sv00001022sd00001635bc06sc04i00
E: PCI_CLASS=60400
E: PCI_ID=1022:1635
E: PCI_SLOT_NAME=0000:00:08.1
E: PCI_SUBSYS_ID=1022:1635
E: SUBSYSTEM=pci
A: ari_enabled=0\n
A: broken_parity_status=0\n
A: class=0x060400\n
H: [encoded data, 8199 characters]
A: consistent_dma_mask_bits=32\n
A: current_link_speed=16.0 GT/s PCIe\n
A: current_link_width=16\n
A: d3cold_allowed=1\n
A: device=0x1635\n
A: dma_mask_bits=32\n
L: driver=../../../bus/pci/drivers/pcieport
A: driver_override=(null)\n
A: enable=2\n
L: firmware_node=../../LNXSYSTM:00/LNXSYBUS:00/PNP0A08:00/device:10
L: iommu=../0000:00:00.2/iommu/ivhd0
L: iommu_group=../../../kernel/iommu_groups/6
A: irq=30\n
A: local_cpulist=0-15\n
A: local_cpus=ffff\n
A: max_link_speed=16.0 GT/s PCIe\n
A: max_link_width=16\n
A: modalias=pci:v00001022d00001635sv00001022sd00001635bc06sc04i00\n
A: msi_bus=1\n
A: msi_irqs/30=msi\n
A: numa_node=-1\n
A: power/autosuspend_delay_ms=100\n
A: power/control=auto\n
A: power/runtime_active_time=6808508\n
A: power/runtime_status=active\n
A: power/runtime_suspended_time=0\n
A: power/wakeup=enabled\n
A: power/wakeup_abort_count=0\n
A: power/wakeup_active=0\n
A: power/wakeup_active_count=0\n
A: power/wakeup_count=0\n
A: power/wakeup_expire_count=0\n
A: power/wakeup_last_time_ms=0\n
A: power/wakeup_max_time_ms=0\n
A: power/wakeup_total_time_ms=0\n
A: power_state=D0\n
A: reset_method=pm\n
A: resource=0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x000000000000c000 0x000000000000cfff 0x0000000000000101\n0x00000000fc200000 0x00000000fc5fffff 0x0000000000000200\n0x00000000d0000000 0x00000000e01fffff 0x0000000000102201\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n
A: revision=0x00\n
A: secondary_bus_number=5\n
A: subordinate_bus_number=5\n
A: subsystem_device=0x1635\n
A: subsystem_vendor=0x1022\n
A: vendor=0x1022\n

