@DEV /dev/bus/usb/001/094
USBDEVFS_GET_CAPABILITIES 0 FD000000
USBDEVFS_REAPURBNDELAY 0 3 1 0 0 2 2 0 4019
 USBDEVFS_REAPURBNDELAY 0 3 131 0 0 2 2 0 0140
USBDEVFS_REAPURBNDELAY 0 3 1 0 0 2 2 0 000C
 USBDEVFS_REAPURBNDELAY 0 3 131 0 0 4 4 0 40009000
USBDEVFS_REAPURBNDELAY 0 3 1 0 0 2 2 0 0009
 USBDEVFS_REAPURBNDELAY 0 3 130 0 0 18432 18432 0 [encoded data, 36864 characters]
 USBDEVFS_REAPURBNDELAY 0 3 130 0 0 18432 18432 0 [encoded data, 36864 characters]
 USBDEVFS_REAPURBNDELAY 0 3 130 0 0 18432 18432 0 [encoded data, 36864 characters]
 USBDEVFS_REAPURBNDELAY 0 3 130 0 0 18432 18432 0 [encoded data, 36864 characters]
 USBDEVFS_REAPURBNDELAY 0 3 130 0 0 18432 18432 0 [encoded data, 36864 characters]
 USBDEVFS_REAPURBNDELAY 0 3 130 0 0 18432 18432 0 [encoded data, 36864 characters]
 USBDEVFS_REAPURBNDELAY 0 3 130 0 0 18432 18432 0 [encoded data, 36864 characters]
 USBDEVFS_REAPURBNDELAY 0 3 130 0 0 18432 18432 0 [encoded data, 36864 characters]
 USBDEVFS_REAPURBNDELAY 0 3 130 0 0 18432 18432 0 [encoded data, 36864 characters]
 USBDEVFS_REAPURBNDELAY 0 3 130 0 0 18432 18432 0 [encoded data, 36864 characters]
 USBDEVFS_REAPURBNDELAY 0 3 130 0 0 18432 18432 0 [encoded data, 36864 characters]
 USBDEVFS_REAPURBNDELAY 0 3 130 0 0 18432 18432 0 [encoded data, 36864 characters]
 USBDEVFS_REAPURBNDELAY 0 3 130 0 0 18432 18432 0 [encoded data, 36864 characters]
 USBDEVFS_REAPURBNDELAY 0 3 130 0 0 18432 18432 0 [encoded data, 36864 characters]
USBDEVFS_REAPURBNDELAY 0 3 1 0 0 2 2 0 4024
 USBDEVFS_REAPURBNDELAY 0 3 131 0 0 2 2 0 2106
 USBDEVFS_REAPURBNDELAY 0 3 131 0 0 2 2 0 20B3
USBDEVFS_REAPURBNDELAY 0 3 1 0 0 2 2 0 4023
 USBDEVFS_REAPURBNDELAY 0 3 131 0 0 1 1 0 01
 USBDEVFS_REAPURBNDELAY 0 3 131 0 0 1 1 0 01
 USBDEVFS_REAPURBNDELAY 0 3 131 0 0 1 1 0 01
 USBDEVFS_REAPURBNDELAY 0 3 131 0 0 1 1 0 01
 USBDEVFS_REAPURBNDELAY 0 3 131 0 0 1 1 0 01
 USBDEVFS_REAPURBNDELAY 0 3 131 0 0 1 1 0 03
USBDEVFS_REAPURBNDELAY 0 3 1 0 0 2 2 0 4031
USBDEVFS_REAPURBNDELAY 0 3 1 0 0 2 2 0 403F
 USBDEVFS_REAPURBNDELAY 0 3 131 0 0 1 1 0 55
 USBDEVFS_REAPURBNDELAY 0 3 131 0 0 1 1 0 55
 USBDEVFS_REAPURBNDELAY 0 3 131 0 0 1 1 0 55
 USBDEVFS_REAPURBNDELAY 0 3 131 0 0 1 1 0 55
 USBDEVFS_REAPURBNDELAY 0 3 131 0 0 1 1 0 55
 USBDEVFS_REAPURBNDELAY 0 3 131 0 0 1 1 0 55
 USBDEVFS_REAPURBNDELAY 0 3 131 0 0 1 1 0 55
 USBDEVFS_REAPURBNDELAY 0 3 131 0 0 1 1 0 55
 USBDEVFS_REAPURBNDELAY 0 3 131 0 0 1 1 0 55
 USBDEVFS_REAPURBNDELAY 0 3 131 0 0 1 1 0 55
 USBDEVFS_REAPURBNDELAY 0 3 131 0 0 1 1 0 55
 USBDEVFS_REAPURBNDELAY 0 3 131 0 0 1 1 0 55
 USBDEVFS_REAPURBNDELAY 0 3 131 -2 0 1 0 0 
USBDEVFS_REAPURBNDELAY 0 3 1 0 0 2 2 0 000B
