P: /devices/pci0000:00/0000:00:14.0/usb3/3-5
N: bus/usb/003/012=12010002FF0000407A1C820581110102030109022700010100A0320904000003FF000000070581020002000705020200020007058303400005
E: BUSNUM=003
E: CURRENT_TAGS=:snap_cups_ippeveprinter:snap_cups_cupsd:
E: DEVNAME=/dev/bus/usb/003/012
E: DEVNUM=012
E: DEVTYPE=usb_device
E: DRIVER=usb
E: ID_BUS=usb
E: ID_MODEL=ETU905A80-E
E: ID_MODEL_ENC=ETU905A80-E
E: ID_MODEL_ID=0582
E: ID_PATH=pci-0000:00:14.0-usb-0:5
E: ID_PATH_TAG=pci-0000_00_14_0-usb-0_5
E: ID_REVISION=1181
E: ID_SERIAL=EGIS_ETU905A80-E_0E7828PBS393
E: ID_SERIAL_SHORT=0E7828PBS393
E: ID_USB_INTERFACES=:ff0000:
E: ID_USB_MODEL=ETU905A80-E
E: ID_USB_MODEL_ENC=ETU905A80-E
E: ID_USB_MODEL_ID=0582
E: ID_USB_REVISION=1181
E: ID_USB_SERIAL=EGIS_ETU905A80-E_0E7828PBS393
E: ID_USB_SERIAL_SHORT=0E7828PBS393
E: ID_USB_VENDOR=EGIS
E: ID_USB_VENDOR_ENC=EGIS
E: ID_USB_VENDOR_ID=1c7a
E: ID_VENDOR=EGIS
E: ID_VENDOR_ENC=EGIS
E: ID_VENDOR_FROM_DATABASE=LighTuning Technology Inc.
E: ID_VENDOR_ID=1c7a
E: MAJOR=189
E: MINOR=267
E: PRODUCT=1c7a/582/1181
E: SUBSYSTEM=usb
E: TAGS=:snap_cups_ippeveprinter:snap_cups_cupsd:
E: TYPE=255/0/0
A: authorized=1\n
A: avoid_reset_quirk=0\n
A: bConfigurationValue=1\n
A: bDeviceClass=ff\n
A: bDeviceProtocol=00\n
A: bDeviceSubClass=00\n
A: bMaxPacketSize0=64\n
A: bMaxPower=100mA\n
A: bNumConfigurations=1\n
A: bNumInterfaces= 1\n
A: bcdDevice=1181\n
A: bmAttributes=a0\n
A: busnum=3\n
A: configuration=
H: descriptors=12010002FF0000407A1C820581110102030109022700010100A0320904000003FF000000070581020002000705020200020007058303400005
A: dev=189:267\n
A: devnum=12\n
A: devpath=5\n
L: driver=../../../../../bus/usb/drivers/usb
L: firmware_node=../../../../LNXSYSTM:00/LNXSYBUS:00/PNP0A08:00/device:51/device:52/device:57
A: idProduct=0582\n
A: idVendor=1c7a\n
A: ltm_capable=no\n
A: manufacturer=EGIS\n
A: maxchild=0\n
A: physical_location/dock=no\n
A: physical_location/horizontal_position=center\n
A: physical_location/lid=no\n
A: physical_location/panel=unknown\n
A: physical_location/vertical_position=center\n
L: port=../3-0:1.0/usb3-port5
A: power/active_duration=1425996\n
A: power/async=enabled\n
A: power/autosuspend=2\n
A: power/autosuspend_delay_ms=2000\n
A: power/connected_duration=1426656\n
A: power/control=on\n
A: power/level=on\n
A: power/persist=0\n
A: power/runtime_active_kids=0\n
A: power/runtime_active_time=1426124\n
A: power/runtime_enabled=forbidden\n
A: power/runtime_status=active\n
A: power/runtime_suspended_time=0\n
A: power/runtime_usage=1\n
A: power/wakeup=disabled\n
A: power/wakeup_abort_count=\n
A: power/wakeup_active=\n
A: power/wakeup_active_count=\n
A: power/wakeup_count=\n
A: power/wakeup_expire_count=\n
A: power/wakeup_last_time_ms=\n
A: power/wakeup_max_time_ms=\n
A: power/wakeup_total_time_ms=\n
A: product=ETU905A80-E\n
A: quirks=0x0\n
A: removable=fixed\n
A: rx_lanes=1\n
A: serial=0E7828PBS393\n
A: speed=480\n
A: tx_lanes=1\n
A: urbnum=2803\n
A: version= 2.00\n

P: /devices/pci0000:00/0000:00:14.0/usb3
N: bus/usb/003/001=12010002090001406B1D020002060302010109021900010100E0000904000001090000000705810304000C
E: BUSNUM=003
E: CURRENT_TAGS=:seat:snap_cups_cupsd:snap_cups_ippeveprinter:
E: DEVNAME=/dev/bus/usb/003/001
E: DEVNUM=001
E: DEVTYPE=usb_device
E: DRIVER=usb
E: ID_AUTOSUSPEND=1
E: ID_BUS=usb
E: ID_FOR_SEAT=usb-pci-0000_00_14_0
E: ID_MODEL=xHCI_Host_Controller
E: ID_MODEL_ENC=xHCI\x20Host\x20Controller
E: ID_MODEL_FROM_DATABASE=2.0 root hub
E: ID_MODEL_ID=0002
E: ID_PATH=pci-0000:00:14.0
E: ID_PATH_TAG=pci-0000_00_14_0
E: ID_REVISION=0602
E: ID_SERIAL=Linux_6.2.0-34-generic_xhci-hcd_xHCI_Host_Controller_0000:00:14.0
E: ID_SERIAL_SHORT=0000:00:14.0
E: ID_USB_INTERFACES=:090000:
E: ID_USB_MODEL=xHCI_Host_Controller
E: ID_USB_MODEL_ENC=xHCI\x20Host\x20Controller
E: ID_USB_MODEL_ID=0002
E: ID_USB_REVISION=0602
E: ID_USB_SERIAL=Linux_6.2.0-34-generic_xhci-hcd_xHCI_Host_Controller_0000:00:14.0
E: ID_USB_SERIAL_SHORT=0000:00:14.0
E: ID_USB_VENDOR=Linux_6.2.0-34-generic_xhci-hcd
E: ID_USB_VENDOR_ENC=Linux\x206.2.0-34-generic\x20xhci-hcd
E: ID_USB_VENDOR_ID=1d6b
E: ID_VENDOR=Linux_6.2.0-34-generic_xhci-hcd
E: ID_VENDOR_ENC=Linux\x206.2.0-34-generic\x20xhci-hcd
E: ID_VENDOR_FROM_DATABASE=Linux Foundation
E: ID_VENDOR_ID=1d6b
E: MAJOR=189
E: MINOR=256
E: PRODUCT=1d6b/2/602
E: SUBSYSTEM=usb
E: TAGS=:snap_cups_cupsd:seat:snap_cups_ippeveprinter:
E: TYPE=9/0/1
A: authorized=1\n
A: authorized_default=1\n
A: avoid_reset_quirk=0\n
A: bConfigurationValue=1\n
A: bDeviceClass=09\n
A: bDeviceProtocol=01\n
A: bDeviceSubClass=00\n
A: bMaxPacketSize0=64\n
A: bMaxPower=0mA\n
A: bNumConfigurations=1\n
A: bNumInterfaces= 1\n
A: bcdDevice=0602\n
A: bmAttributes=e0\n
A: busnum=3\n
A: configuration=
H: descriptors=12010002090001406B1D020002060302010109021900010100E0000904000001090000000705810304000C
A: dev=189:256\n
A: devnum=1\n
A: devpath=0\n
L: driver=../../../../bus/usb/drivers/usb
L: firmware_node=../../../LNXSYSTM:00/LNXSYBUS:00/PNP0A08:00/device:51/device:52
A: idProduct=0002\n
A: idVendor=1d6b\n
A: interface_authorized_default=1\n
A: ltm_capable=no\n
A: manufacturer=Linux 6.2.0-34-generic xhci-hcd\n
A: maxchild=12\n
A: power/active_duration=337953872\n
A: power/async=enabled\n
A: power/autosuspend=0\n
A: power/autosuspend_delay_ms=0\n
A: power/connected_duration=337978524\n
A: power/control=auto\n
A: power/level=auto\n
A: power/runtime_active_kids=1\n
A: power/runtime_active_time=337962424\n
A: power/runtime_enabled=enabled\n
A: power/runtime_status=active\n
A: power/runtime_suspended_time=616\n
A: power/runtime_usage=0\n
A: power/wakeup=disabled\n
A: power/wakeup_abort_count=\n
A: power/wakeup_active=\n
A: power/wakeup_active_count=\n
A: power/wakeup_count=\n
A: power/wakeup_expire_count=\n
A: power/wakeup_last_time_ms=\n
A: power/wakeup_max_time_ms=\n
A: power/wakeup_total_time_ms=\n
A: product=xHCI Host Controller\n
A: quirks=0x0\n
A: removable=unknown\n
A: rx_lanes=1\n
A: serial=0000:00:14.0\n
A: speed=480\n
A: tx_lanes=1\n
A: urbnum=4969\n
A: version= 2.00\n

P: /devices/pci0000:00/0000:00:14.0
E: DRIVER=xhci_hcd
E: ID_MODEL_FROM_DATABASE=Alder Lake PCH USB 3.2 xHCI Host Controller
E: ID_PCI_CLASS_FROM_DATABASE=Serial bus controller
E: ID_PCI_INTERFACE_FROM_DATABASE=XHCI
E: ID_PCI_SUBCLASS_FROM_DATABASE=USB controller
E: ID_VENDOR_FROM_DATABASE=Intel Corporation
E: MODALIAS=pci:v00008086d000051EDsv0000144Dsd0000C870bc0Csc03i30
E: PCI_CLASS=C0330
E: PCI_ID=8086:51ED
E: PCI_SLOT_NAME=0000:00:14.0
E: PCI_SUBSYS_ID=144D:C870
E: SUBSYSTEM=pci
A: ari_enabled=0\n
A: broken_parity_status=0\n
A: class=0x0c0330\n
H: config=8680ED51060490020130030C000080000400161D6000000000000000000000000000000000000000000000004D1470C8000000007000000000000000FF010000FD0134A089C27F8000000000000000003F6DD80F000000000000000000000000316000000000000000000000000000000180C2C1080000000000000000000000059087007805E0FE000000000000000009B014F01000400100000000C10A080000080E00001800008F50020000010000090000018680C00009001014000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000B50F010112000000
A: consistent_dma_mask_bits=64\n
A: d3cold_allowed=1\n
A: dbc=disabled\n
A: device=0x51ed\n
A: dma_mask_bits=64\n
L: driver=../../../bus/pci/drivers/xhci_hcd
A: driver_override=(null)\n
A: enable=1\n
L: firmware_node=../../LNXSYSTM:00/LNXSYBUS:00/PNP0A08:00/device:51
A: index=7\n
L: iommu=../../virtual/iommu/dmar1
L: iommu_group=../../../kernel/iommu_groups/8
A: irq=145\n
A: label=Onboard - Other\n
A: local_cpulist=0-15\n
A: local_cpus=ffff\n
A: modalias=pci:v00008086d000051EDsv0000144Dsd0000C870bc0Csc03i30\n
A: msi_bus=1\n
A: msi_irqs/145=msi\n
A: numa_node=-1\n
A: pools=poolinfo - 0.1\nbuffer-2048         0    0 2048  0\nbuffer-512          0    0  512  0\nbuffer-128          0    0  128  0\nbuffer-32           0    0   32  0\nxHCI 1KB stream ctx arrays    0    0 1024  0\nxHCI 256 byte stream ctx arrays    0    0  256  0\nxHCI input/output contexts    6    9 2112  9\nxHCI ring segments   26   34 4096 34\nbuffer-2048         0    0 2048  0\nbuffer-512          0    0  512  0\nbuffer-128          0   32  128  1\nbuffer-32           0    0   32  0\n
A: power/async=enabled\n
A: power/control=auto\n
A: power/runtime_active_kids=1\n
A: power/runtime_active_time=337964621\n
A: power/runtime_enabled=enabled\n
A: power/runtime_status=active\n
A: power/runtime_suspended_time=438\n
A: power/runtime_usage=0\n
A: power/wakeup=enabled\n
A: power/wakeup_abort_count=0\n
A: power/wakeup_active=0\n
A: power/wakeup_active_count=7\n
A: power/wakeup_count=0\n
A: power/wakeup_expire_count=7\n
A: power/wakeup_last_time_ms=336554844\n
A: power/wakeup_max_time_ms=105\n
A: power/wakeup_total_time_ms=721\n
A: power_state=D0\n
A: resource=0x000000601d160000 0x000000601d16ffff 0x0000000000140204\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n
A: revision=0x01\n
A: subsystem_device=0xc870\n
A: subsystem_vendor=0x144d\n
A: vendor=0x8086\n

