P: /devices/pci0000:00/0000:00:14.0/usb1/1-10
N: bus/usb/001/050=1201000200000040BA050A000301010203010902200001010080640904000002FFFFFF000705810340000807058202400000
E: DEVNAME=/dev/bus/usb/001/050
E: DEVTYPE=usb_device
E: DRIVER=usb
E: PRODUCT=5ba/a/103
E: TYPE=0/0/0
E: BUSNUM=001
E: DEVNUM=050
E: MAJOR=189
E: MINOR=49
E: SUBSYSTEM=usb
E: ID_VENDOR=DigitalPersona__Inc.
E: ID_VENDOR_ENC=DigitalPersona\x2c\x20Inc.
E: ID_VENDOR_ID=05ba
E: ID_MODEL=U.are.U®_4500_Fingerprint_Reader
E: ID_MODEL_ENC=U.are.U®\x204500\x20Fingerprint\x20Reader
E: ID_MODEL_ID=000a
E: ID_REVISION=0103
E: ID_SERIAL=DigitalPersona__Inc._U.are.U®_4500_Fingerprint_Reader__FB0B9071-2E08-7742-BC16-2FAA247CEF66_
E: ID_SERIAL_SHORT=_FB0B9071-2E08-7742-BC16-2FAA247CEF66_
E: ID_BUS=usb
E: ID_USB_INTERFACES=:ffffff:
E: ID_VENDOR_FROM_DATABASE=DigitalPersona, Inc.
E: ID_AUTOSUSPEND=1
E: ID_MODEL_FROM_DATABASE=Fingerprint Reader
E: ID_PATH=pci-0000:00:14.0-usb-0:10
E: ID_PATH_TAG=pci-0000_00_14_0-usb-0_10
E: LIBFPRINT_DRIVER=Digital Persona U.are.U 4000/4000B/4500
E: ID_FOR_SEAT=usb-pci-0000_00_14_0-usb-0_10
E: TAGS=:seat:
E: CURRENT_TAGS=:seat:
A: authorized=1\n
A: avoid_reset_quirk=0\n
A: bConfigurationValue=1\n
A: bDeviceClass=00\n
A: bDeviceProtocol=00\n
A: bDeviceSubClass=00\n
A: bMaxPacketSize0=64\n
A: bMaxPower=200mA\n
A: bNumConfigurations=1\n
A: bNumInterfaces= 1\n
A: bcdDevice=0103\n
A: bmAttributes=80\n
A: busnum=1\n
A: configuration=
H: descriptors=1201000200000040BA050A000301010203010902200001010080640904000002FFFFFF000705810340000807058202400000
A: dev=189:49\n
A: devnum=50\n
A: devpath=10\n
L: driver=../../../../../bus/usb/drivers/usb
L: firmware_node=../../../../LNXSYSTM:00/LNXSYBUS:00/PNP0A08:00/device:4c/device:4d/device:57
A: idProduct=000a\n
A: idVendor=05ba\n
A: ltm_capable=no\n
A: manufacturer=DigitalPersona, Inc.\n
A: maxchild=0\n
L: port=../1-0:1.0/usb1-port10
A: power/active_duration=2761\n
A: power/autosuspend=2\n
A: power/autosuspend_delay_ms=2000\n
A: power/connected_duration=118841\n
A: power/control=auto\n
A: power/level=auto\n
A: power/persist=0\n
A: power/runtime_active_time=2616\n
A: power/runtime_status=active\n
A: power/runtime_suspended_time=115982\n
A: product=U.are.U\302\256 4500 Fingerprint Reader\n
A: quirks=0x0\n
A: removable=removable\n
A: rx_lanes=1\n
A: serial={FB0B9071-2E08-7742-BC16-2FAA247CEF66}\n
A: speed=12\n
A: tx_lanes=1\n
A: urbnum=13\n
A: version= 2.00\n

P: /devices/pci0000:00/0000:00:14.0/usb1
N: bus/usb/001/001=12010002090001406B1D020013050302010109021900010100E0000904000001090000000705810304000C
E: DEVNAME=/dev/bus/usb/001/001
E: DEVTYPE=usb_device
E: DRIVER=usb
E: PRODUCT=1d6b/2/513
E: TYPE=9/0/1
E: BUSNUM=001
E: DEVNUM=001
E: MAJOR=189
E: MINOR=0
E: SUBSYSTEM=usb
E: ID_VENDOR=Linux_5.13.12-200.fc34.x86_64_xhci-hcd
E: ID_VENDOR_ENC=Linux\x205.13.12-200.fc34.x86_64\x20xhci-hcd
E: ID_VENDOR_ID=1d6b
E: ID_MODEL=xHCI_Host_Controller
E: ID_MODEL_ENC=xHCI\x20Host\x20Controller
E: ID_MODEL_ID=0002
E: ID_REVISION=0513
E: ID_SERIAL=Linux_5.13.12-200.fc34.x86_64_xhci-hcd_xHCI_Host_Controller_0000:00:14.0
E: ID_SERIAL_SHORT=0000:00:14.0
E: ID_BUS=usb
E: ID_USB_INTERFACES=:090000:
E: ID_VENDOR_FROM_DATABASE=Linux Foundation
E: ID_AUTOSUSPEND=1
E: ID_MODEL_FROM_DATABASE=2.0 root hub
E: ID_PATH=pci-0000:00:14.0
E: ID_PATH_TAG=pci-0000_00_14_0
E: ID_FOR_SEAT=usb-pci-0000_00_14_0
E: TAGS=:seat:
E: CURRENT_TAGS=:seat:
A: authorized=1\n
A: authorized_default=1\n
A: avoid_reset_quirk=0\n
A: bConfigurationValue=1\n
A: bDeviceClass=09\n
A: bDeviceProtocol=01\n
A: bDeviceSubClass=00\n
A: bMaxPacketSize0=64\n
A: bMaxPower=0mA\n
A: bNumConfigurations=1\n
A: bNumInterfaces= 1\n
A: bcdDevice=0513\n
A: bmAttributes=e0\n
A: busnum=1\n
A: configuration=
H: descriptors=12010002090001406B1D020013050302010109021900010100E0000904000001090000000705810304000C
A: dev=189:0\n
A: devnum=1\n
A: devpath=0\n
L: driver=../../../../bus/usb/drivers/usb
L: firmware_node=../../../LNXSYSTM:00/LNXSYBUS:00/PNP0A08:00/device:4c/device:4d
A: idProduct=0002\n
A: idVendor=1d6b\n
A: interface_authorized_default=1\n
A: ltm_capable=no\n
A: manufacturer=Linux 5.13.12-200.fc34.x86_64 xhci-hcd\n
A: maxchild=16\n
A: power/active_duration=837797629\n
A: power/autosuspend=0\n
A: power/autosuspend_delay_ms=0\n
A: power/connected_duration=837797629\n
A: power/control=auto\n
A: power/level=auto\n
A: power/runtime_active_time=837797626\n
A: power/runtime_status=active\n
A: power/runtime_suspended_time=0\n
A: power/wakeup=disabled\n
A: power/wakeup_abort_count=\n
A: power/wakeup_active=\n
A: power/wakeup_active_count=\n
A: power/wakeup_count=\n
A: power/wakeup_expire_count=\n
A: power/wakeup_last_time_ms=\n
A: power/wakeup_max_time_ms=\n
A: power/wakeup_total_time_ms=\n
A: product=xHCI Host Controller\n
A: quirks=0x0\n
A: removable=unknown\n
A: rx_lanes=1\n
A: serial=0000:00:14.0\n
A: speed=480\n
A: tx_lanes=1\n
A: urbnum=1498\n
A: version= 2.00\n

P: /devices/pci0000:00/0000:00:14.0
E: DRIVER=xhci_hcd
E: PCI_CLASS=C0330
E: PCI_ID=8086:A36D
E: PCI_SUBSYS_ID=17AA:312A
E: PCI_SLOT_NAME=0000:00:14.0
E: MODALIAS=pci:v00008086d0000A36Dsv000017AAsd0000312Abc0Csc03i30
E: SUBSYSTEM=pci
E: ID_PCI_CLASS_FROM_DATABASE=Serial bus controller
E: ID_PCI_SUBCLASS_FROM_DATABASE=USB controller
E: ID_PCI_INTERFACE_FROM_DATABASE=XHCI
E: ID_VENDOR_FROM_DATABASE=Intel Corporation
E: ID_MODEL_FROM_DATABASE=Cannon Lake PCH USB 3.1 xHCI Host Controller
A: ari_enabled=0\n
A: broken_parity_status=0\n
A: class=0x0c0330\n
H: config=86806DA3060490021030030C00008000040032B1000000000000000000000000000000000000000000000000AA172A31000000007000000000000000FF010000FD0134808FC6FF8300000000000000007F6DDC0F000000009A1CF40100000000316000000000000000000000000000000180C2C1080000000000000000000000059087009802E0FE0000000000000000090014F01000400100000000C10A080000080E00001800008F400200000100006000000008020000010000000400000090000000001800000005000000000000000300000C0000004000000080000000030000000000000000000000000000000000000000000000B50F110112000000
A: consistent_dma_mask_bits=64\n
A: d3cold_allowed=1\n
A: dbc=disabled\n
A: device=0xa36d\n
A: dma_mask_bits=64\n
L: driver=../../../bus/pci/drivers/xhci_hcd
A: driver_override=(null)\n
A: enable=1\n
L: firmware_node=../../LNXSYSTM:00/LNXSYBUS:00/PNP0A08:00/device:4c
A: index=3\n
A: irq=125\n
A: label=Onboard - Other\n
A: local_cpulist=0-5\n
A: local_cpus=3f\n
A: modalias=pci:v00008086d0000A36Dsv000017AAsd0000312Abc0Csc03i30\n
A: msi_bus=1\n
A: msi_irqs/125=msi\n
A: numa_node=-1\n
A: pools=poolinfo - 0.1\nbuffer-2048         0    0 2048  0\nbuffer-512          0    0  512  0\nbuffer-128          0    0  128  0\nbuffer-32           0    0   32  0\nxHCI 1KB stream ctx arrays    0    0 1024  0\nxHCI 256 byte stream ctx arrays    0    0  256  0\nxHCI input/output contexts   15   20 2112 20\nxHCI ring segments   46   76 4096 76\nbuffer-2048         0   32 2048 16\nbuffer-512          0   32  512  4\nbuffer-128          3   32  128  1\nbuffer-32           0  128   32  1\n
A: power/control=on\n
A: power/runtime_active_time=837797789\n
A: power/runtime_status=active\n
A: power/runtime_suspended_time=0\n
A: power/wakeup=enabled\n
A: power/wakeup_abort_count=0\n
A: power/wakeup_active=0\n
A: power/wakeup_active_count=67\n
A: power/wakeup_count=0\n
A: power/wakeup_expire_count=67\n
A: power/wakeup_last_time_ms=835747082\n
A: power/wakeup_max_time_ms=108\n
A: power/wakeup_total_time_ms=6974\n
A: power_state=D0\n
A: resource=0x00000000b1320000 0x00000000b132ffff 0x0000000000140204\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n
A: revision=0x10\n
A: subsystem_device=0x312a\n
A: subsystem_vendor=0x17aa\n
A: vendor=0x8086\n

