P: /devices/pci0000:00/0000:00:14.0/usb2/2-6
N: bus/usb/002/017=12011001FF11FF088A13170078000000010109022E00010100A0320904000004FF00000007050102400000070581024000000705820240000007058303080004
E: DEVNAME=/dev/bus/usb/002/017
E: DEVTYPE=usb_device
E: DRIVER=usb
E: PRODUCT=138a/17/78
E: TYPE=255/17/255
E: BUSNUM=002
E: DEVNUM=017
E: MAJOR=189
E: MINOR=144
E: SUBSYSTEM=usb
E: ID_VENDOR=138a
E: ID_VENDOR_ENC=138a
E: ID_VENDOR_ID=138a
E: ID_MODEL=0017
E: ID_MODEL_ENC=0017
E: ID_MODEL_ID=0017
E: ID_REVISION=0078
E: ID_SERIAL=138a_0017_6c3b5712a6c0
E: ID_SERIAL_SHORT=6c3b5712a6c0
E: ID_BUS=usb
E: ID_USB_INTERFACES=:ff0000:
E: ID_VENDOR_FROM_DATABASE=Validity Sensors, Inc.
E: ID_MODEL_FROM_DATABASE=VFS 5011 fingerprint sensor
A: authorized=1
A: avoid_reset_quirk=0
A: bConfigurationValue=1
A: bDeviceClass=ff
A: bDeviceProtocol=ff
A: bDeviceSubClass=11
A: bMaxPacketSize0=8
A: bMaxPower=100mA
A: bNumConfigurations=1
A: bNumInterfaces= 1
A: bcdDevice=0078
A: bmAttributes=a0
A: busnum=2\n
A: configuration=
H: descriptors=12011001FF11FF088A13170078000000010109022E00010100A0320904000004FF00000007050102400000070581024000000705820240000007058303080004
A: dev=189:144
A: devnum=17\n
A: devpath=6
L: driver=../../../../../bus/usb/drivers/usb
A: idProduct=0017
A: idVendor=138a
A: ltm_capable=no
A: maxchild=0
L: port=../2-0:1.0/usb2-port6
A: power/active_duration=624952
A: power/async=enabled
A: power/autosuspend=2
A: power/autosuspend_delay_ms=2000
A: power/connected_duration=624952
A: power/control=on
A: power/level=on
A: power/persist=1
A: power/runtime_active_kids=0
A: power/runtime_active_time=624676
A: power/runtime_enabled=forbidden
A: power/runtime_status=active
A: power/runtime_suspended_time=0
A: power/runtime_usage=1
A: power/wakeup=disabled
A: power/wakeup_abort_count=
A: power/wakeup_active=
A: power/wakeup_active_count=
A: power/wakeup_count=
A: power/wakeup_expire_count=
A: power/wakeup_last_time_ms=
A: power/wakeup_max_time_ms=
A: power/wakeup_total_time_ms=
A: quirks=0x0
A: removable=fixed
A: rx_lanes=1
A: serial=6c3b5712a6c0
A: speed=12
A: tx_lanes=1
A: urbnum=7
A: version= 1.10

P: /devices/pci0000:00/0000:00:14.0/usb2
N: bus/usb/002/001=12010002090001406B1D020011050302010109021900010100E0000904000001090000000705810304000C
E: DEVNAME=/dev/bus/usb/002/001
E: DEVTYPE=usb_device
E: DRIVER=usb
E: PRODUCT=1d6b/2/511
E: TYPE=9/0/1
E: BUSNUM=002
E: DEVNUM=001
E: MAJOR=189
E: MINOR=0
E: SUBSYSTEM=usb
E: ID_VENDOR=Linux_5.11.2-arch1-1_xhci-hcd
E: ID_VENDOR_ENC=Linux\x205.11.2-arch1-1\x20xhci-hcd
E: ID_VENDOR_ID=1d6b
E: ID_MODEL=xHCI_Host_Controller
E: ID_MODEL_ENC=xHCI\x20Host\x20Controller
E: ID_MODEL_ID=0002
E: ID_REVISION=0511
E: ID_SERIAL=Linux_5.11.2-arch1-1_xhci-hcd_xHCI_Host_Controller_0000:00:14.0
E: ID_SERIAL_SHORT=0000:00:14.0
E: ID_BUS=usb
E: ID_USB_INTERFACES=:090000:
E: ID_VENDOR_FROM_DATABASE=Linux Foundation
E: ID_AUTOSUSPEND=1
E: ID_MODEL_FROM_DATABASE=2.0 root hub
E: ID_PATH=pci-0000:00:14.0
E: ID_PATH_TAG=pci-0000_00_14_0
E: ID_FOR_SEAT=usb-pci-0000_00_14_0
E: TAGS=:seat:
E: CURRENT_TAGS=:seat:
A: authorized=1\n
A: authorized_default=1\n
A: avoid_reset_quirk=0\n
A: bConfigurationValue=1\n
A: bDeviceClass=09\n
A: bDeviceProtocol=01\n
A: bDeviceSubClass=00\n
A: bMaxPacketSize0=64\n
A: bMaxPower=0mA\n
A: bNumConfigurations=1\n
A: bNumInterfaces= 1\n
A: bcdDevice=0511\n
A: bmAttributes=e0\n
A: busnum=1\n
A: configuration=
H: descriptors=12010002090001406B1D020011050302010109021900010100E0000904000001090000000705810304000C
A: dev=189:0\n
A: devnum=1\n
A: devpath=0\n
L: driver=../../../../bus/usb/drivers/usb
L: firmware_node=../../../LNXSYSTM:00/LNXSYBUS:00/PNP0A08:00/device:4c/device:4d
A: idProduct=0002\n
A: idVendor=1d6b\n
A: interface_authorized_default=1\n
A: ltm_capable=no\n
A: manufacturer=Linux 5.11.2-arch1-1 xhci-hcd\n
A: maxchild=16\n
A: power/active_duration=3289930\n
A: power/autosuspend=0\n
A: power/autosuspend_delay_ms=0\n
A: power/connected_duration=34389654\n
A: power/control=auto\n
A: power/level=auto\n
A: power/runtime_active_time=3289845\n
A: power/runtime_status=active\n
A: power/runtime_suspended_time=31099805\n
A: power/wakeup=disabled\n
A: power/wakeup_abort_count=\n
A: power/wakeup_active=\n
A: power/wakeup_active_count=\n
A: power/wakeup_count=\n
A: power/wakeup_expire_count=\n
A: power/wakeup_last_time_ms=\n
A: power/wakeup_max_time_ms=\n
A: power/wakeup_total_time_ms=\n
A: product=xHCI Host Controller\n
A: quirks=0x0\n
A: removable=unknown\n
A: rx_lanes=1\n
A: serial=0000:00:14.0\n
A: speed=480\n
A: tx_lanes=1\n
A: urbnum=2355\n
A: version= 2.00\n

P: /devices/pci0000:00/0000:00:14.0
E: DRIVER=xhci_hcd
E: PCI_CLASS=C0330
E: PCI_ID=8086:A12F
E: PCI_SUBSYS_ID=1028:07BE
E: PCI_SLOT_NAME=0000:00:14.0
E: MODALIAS=pci:v00008086d0000A12Fsv00001028sd000007BEbc0Csc03i30
E: SUBSYSTEM=pci
E: ID_PCI_CLASS_FROM_DATABASE=Serial bus controller
E: ID_PCI_SUBCLASS_FROM_DATABASE=USB controller
E: ID_PCI_INTERFACE_FROM_DATABASE=XHCI
E: ID_VENDOR_FROM_DATABASE=Intel Corporation
E: ID_MODEL_FROM_DATABASE=100 Series/C230 Series Chipset Family USB 3.0 xHCI Controller
A: ari_enabled=0\n
A: broken_parity_status=0\n
A: class=0x0c0330\n
H: config=86802FA1060490023130030C000080000400D1ED0000000000000000000000000000000000000000000000002810BE07000000007000000000000000FF010000
A: consistent_dma_mask_bits=64\n
A: d3cold_allowed=1\n
A: device=0xa12f\n
A: dma_mask_bits=64\n
L: driver=../../../bus/pci/drivers/xhci_hcd
A: driver_override=(null)\n
A: enable=1\n
L: firmware_node=../../LNXSYSTM:00/LNXSYBUS:00/PNP0A08:00/device:4c
L: iommu=../../virtual/iommu/dmar1
L: iommu_group=../../../kernel/iommu_groups/4
A: irq=143\n
A: local_cpulist=0-7\n
A: local_cpus=ff\n
A: modalias=pci:v00008086d0000A12Fsv00001028sd000007BEbc0Csc03i30\n
A: msi_bus=1\n
A: msi_irqs/143=msi\n
A: numa_node=-1\n
A: pools=poolinfo - 0.1\nbuffer-2048         0    0 2048  0\nbuffer-512          0    0  512  0\nbuffer-128          0    0  128  0\nbuffer-32           0    0   32  0\nxHCI 1KB stream ctx arrays    0    0 1024  0\nxHCI 256 byte stream ctx arrays    0    0  256  0\nxHCI input/output contexts    7   10 2112 10\nxHCI ring segments   30   38 4096 38\nbuffer-2048         0    0 2048  0\nbuffer-512          0    0  512  0\nbuffer-128          0    0  128  0\nbuffer-32           0    0   32  0\n
A: power/control=on\n
A: power/runtime_active_time=34390988\n
A: power/runtime_status=active\n
A: power/runtime_suspended_time=0\n
A: power/wakeup=enabled\n
A: power/wakeup_abort_count=0\n
A: power/wakeup_active=0\n
A: power/wakeup_active_count=0\n
A: power/wakeup_count=0\n
A: power/wakeup_expire_count=0\n
A: power/wakeup_last_time_ms=0\n
A: power/wakeup_max_time_ms=0\n
A: power/wakeup_total_time_ms=0\n
A: power_state=D0\n
A: resource=0x00000000edd10000 0x00000000edd1ffff 0x0000000000140204\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n
A: revision=0x31\n
A: subsystem_device=0x07be\n
A: subsystem_vendor=0x1028\n
A: vendor=0x8086\n

