P: /devices/pci0000:00/0000:00:1c.4/0000:0b:00.0/usb3/3-1/3-1.4
N: bus/usb/003/006=1201100100000040082879D900020102030109022000010100A0320904000002DCA0B0000705020240000007058102400000
E: DEVNAME=/dev/bus/usb/003/006
E: DEVTYPE=usb_device
E: DRIVER=usb
E: PRODUCT=2808/d979/200
E: TYPE=0/0/0
E: BUSNUM=003
E: DEVNUM=006
E: MAJOR=189
E: MINOR=261
E: SUBSYSTEM=usb
E: ID_VENDOR=CCore
E: ID_VENDOR_ENC=CCore
E: ID_VENDOR_ID=2808
E: ID_MODEL=FocalTech_FT9349_ESS
E: ID_MODEL_ENC=FocalTech\x20FT9349\x20ESS
E: ID_MODEL_ID=d979
E: ID_REVISION=0200
E: ID_SERIAL=CCore_FocalTech_FT9349_ESS_1234567890ABCDEF
E: ID_SERIAL_SHORT=1234567890ABCDEF
E: ID_BUS=usb
E: ID_USB_INTERFACES=:dca0b0:
E: ID_PATH=pci-0000:0b:00.0-usb-0:1.4
E: ID_PATH_TAG=pci-0000_0b_00_0-usb-0_1_4
A: authorized=1
A: avoid_reset_quirk=0
A: bConfigurationValue=1
A: bDeviceClass=00
A: bDeviceProtocol=00
A: bDeviceSubClass=00
A: bMaxPacketSize0=64
A: bMaxPower=100mA
A: bNumConfigurations=1
A: bNumInterfaces= 1
A: bcdDevice=0200
A: bmAttributes=a0
A: busnum=3
A: configuration=
H: descriptors=1201100100000040082879D900020102030109022000010100A0320904000002DCA0B0000705020240000007058102400000
A: dev=189:261
A: devnum=6
A: devpath=1.4
L: driver=../../../../../../../bus/usb/drivers/usb
A: idProduct=d979
A: idVendor=2808
A: ltm_capable=no
A: manufacturer=CCore
A: maxchild=0
L: port=../3-1:1.0/3-1-port4
A: power/active_duration=130884
A: power/async=enabled
A: power/autosuspend=2
A: power/autosuspend_delay_ms=2000
A: power/connected_duration=2778952
A: power/control=auto
A: power/level=auto
A: power/persist=0
A: power/runtime_active_kids=0
A: power/runtime_active_time=131747
A: power/runtime_enabled=enabled
A: power/runtime_status=active
A: power/runtime_suspended_time=2647026
A: power/runtime_usage=0
A: power/wakeup=disabled
A: power/wakeup_abort_count=
A: power/wakeup_active=
A: power/wakeup_active_count=
A: power/wakeup_count=
A: power/wakeup_expire_count=
A: power/wakeup_last_time_ms=
A: power/wakeup_max_time_ms=
A: power/wakeup_total_time_ms=
A: product=FocalTech FT9349 ESS
A: quirks=0x0
A: removable=unknown
A: rx_lanes=1
A: serial=1234567890ABCDEF
A: speed=12
A: tx_lanes=1
A: urbnum=1922
A: version= 1.10

P: /devices/pci0000:00/0000:00:1c.4/0000:0b:00.0/usb3/3-1
N: bus/usb/003/002=1201000209000140E305080636850001000109021900010100E0320904000001090000000705810301000C
E: DEVNAME=/dev/bus/usb/003/002
E: DEVTYPE=usb_device
E: DRIVER=usb
E: PRODUCT=5e3/608/8536
E: TYPE=9/0/1
E: BUSNUM=003
E: DEVNUM=002
E: MAJOR=189
E: MINOR=257
E: SUBSYSTEM=usb
E: ID_VENDOR=05e3
E: ID_VENDOR_ENC=05e3
E: ID_VENDOR_ID=05e3
E: ID_MODEL=USB2.0_Hub
E: ID_MODEL_ENC=USB2.0\x20Hub
E: ID_MODEL_ID=0608
E: ID_REVISION=8536
E: ID_SERIAL=05e3_USB2.0_Hub
E: ID_BUS=usb
E: ID_USB_INTERFACES=:090000:
E: ID_VENDOR_FROM_DATABASE=Genesys Logic, Inc.
E: ID_MODEL_FROM_DATABASE=Hub
E: ID_PATH=pci-0000:0b:00.0-usb-0:1
E: ID_PATH_TAG=pci-0000_0b_00_0-usb-0_1
E: ID_FOR_SEAT=usb-pci-0000_0b_00_0-usb-0_1
E: TAGS=:seat:
A: authorized=1
A: avoid_reset_quirk=0
A: bConfigurationValue=1
A: bDeviceClass=09
A: bDeviceProtocol=01
A: bDeviceSubClass=00
A: bMaxPacketSize0=64
A: bMaxPower=100mA
A: bNumConfigurations=1
A: bNumInterfaces= 1
A: bcdDevice=8536
A: bmAttributes=e0
A: busnum=3
A: configuration=
H: descriptors=1201000209000140E305080636850001000109021900010100E0320904000001090000000705810301000C
A: dev=189:257
A: devnum=2
A: devpath=1
L: driver=../../../../../../bus/usb/drivers/usb
A: idProduct=0608
A: idVendor=05e3
A: ltm_capable=no
A: maxchild=4
L: port=../3-0:1.0/usb3-port1
A: power/active_duration=6193132
A: power/async=enabled
A: power/autosuspend=0
A: power/autosuspend_delay_ms=0
A: power/connected_duration=6193132
A: power/control=auto
A: power/level=auto
A: power/runtime_active_kids=3
A: power/runtime_active_time=6192633
A: power/runtime_enabled=enabled
A: power/runtime_status=active
A: power/runtime_suspended_time=0
A: power/runtime_usage=0
A: power/wakeup=disabled
A: power/wakeup_abort_count=
A: power/wakeup_active=
A: power/wakeup_active_count=
A: power/wakeup_count=
A: power/wakeup_expire_count=
A: power/wakeup_last_time_ms=
A: power/wakeup_max_time_ms=
A: power/wakeup_total_time_ms=
A: product=USB2.0 Hub
A: quirks=0x0
A: removable=unknown
A: rx_lanes=1
A: speed=480
A: tx_lanes=1
A: urbnum=619
A: version= 2.00

P: /devices/pci0000:00/0000:00:1c.4/0000:0b:00.0/usb3
N: bus/usb/003/001=12010002090001406B1D020015050302010109021900010100E0000904000001090000000705810304000C
E: DEVNAME=/dev/bus/usb/003/001
E: DEVTYPE=usb_device
E: DRIVER=usb
E: PRODUCT=1d6b/2/515
E: TYPE=9/0/1
E: BUSNUM=003
E: DEVNUM=001
E: MAJOR=189
E: MINOR=256
E: SUBSYSTEM=usb
E: ID_VENDOR=Linux_5.15.0-52-generic_xhci-hcd
E: ID_VENDOR_ENC=Linux\x205.15.0-52-generic\x20xhci-hcd
E: ID_VENDOR_ID=1d6b
E: ID_MODEL=xHCI_Host_Controller
E: ID_MODEL_ENC=xHCI\x20Host\x20Controller
E: ID_MODEL_ID=0002
E: ID_REVISION=0515
E: ID_SERIAL=Linux_5.15.0-52-generic_xhci-hcd_xHCI_Host_Controller_0000:0b:00.0
E: ID_SERIAL_SHORT=0000:0b:00.0
E: ID_BUS=usb
E: ID_USB_INTERFACES=:090000:
E: ID_VENDOR_FROM_DATABASE=Linux Foundation
E: ID_MODEL_FROM_DATABASE=2.0 root hub
E: ID_PATH=pci-0000:0b:00.0
E: ID_PATH_TAG=pci-0000_0b_00_0
E: ID_FOR_SEAT=usb-pci-0000_0b_00_0
E: TAGS=:seat:
A: authorized=1
A: authorized_default=1
A: avoid_reset_quirk=0
A: bConfigurationValue=1
A: bDeviceClass=09
A: bDeviceProtocol=01
A: bDeviceSubClass=00
A: bMaxPacketSize0=64
A: bMaxPower=0mA
A: bNumConfigurations=1
A: bNumInterfaces= 1
A: bcdDevice=0515
A: bmAttributes=e0
A: busnum=3
A: configuration=
H: descriptors=12010002090001406B1D020015050302010109021900010100E0000904000001090000000705810304000C
A: dev=189:256
A: devnum=1
A: devpath=0
L: driver=../../../../../bus/usb/drivers/usb
A: idProduct=0002
A: idVendor=1d6b
A: interface_authorized_default=1
A: ltm_capable=no
A: manufacturer=Linux 5.15.0-52-generic xhci-hcd
A: maxchild=2
A: power/active_duration=6193348
A: power/async=enabled
A: power/autosuspend=0
A: power/autosuspend_delay_ms=0
A: power/connected_duration=6193348
A: power/control=auto
A: power/level=auto
A: power/runtime_active_kids=1
A: power/runtime_active_time=6193145
A: power/runtime_enabled=enabled
A: power/runtime_status=active
A: power/runtime_suspended_time=0
A: power/runtime_usage=0
A: power/wakeup=disabled
A: power/wakeup_abort_count=
A: power/wakeup_active=
A: power/wakeup_active_count=
A: power/wakeup_count=
A: power/wakeup_expire_count=
A: power/wakeup_last_time_ms=
A: power/wakeup_max_time_ms=
A: power/wakeup_total_time_ms=
A: product=xHCI Host Controller
A: quirks=0x0
A: removable=unknown
A: rx_lanes=1
A: serial=0000:0b:00.0
A: speed=480
A: tx_lanes=1
A: urbnum=36
A: version= 2.00

P: /devices/pci0000:00/0000:00:1c.4/0000:0b:00.0
E: DRIVER=xhci_hcd
E: PCI_CLASS=C0330
E: PCI_ID=104C:8241
E: PCI_SUBSYS_ID=1028:050F
E: PCI_SLOT_NAME=0000:0b:00.0
E: MODALIAS=pci:v0000104Cd00008241sv00001028sd0000050Fbc0Csc03i30
E: SUBSYSTEM=pci
E: ID_PCI_CLASS_FROM_DATABASE=Serial bus controller
E: ID_PCI_SUBCLASS_FROM_DATABASE=USB controller
E: ID_PCI_INTERFACE_FROM_DATABASE=XHCI
E: ID_VENDOR_FROM_DATABASE=Texas Instruments
E: ID_MODEL_FROM_DATABASE=TUSB73x0 SuperSpeed USB 3.0 xHCI Host Controller
A: aer_dev_correctable=RxErr 0\nBadTLP 0\nBadDLLP 0\nRollover 0\nTimeout 0\nNonFatalErr 0\nCorrIntErr 0\nHeaderOF 0\nTOTAL_ERR_COR 0
A: aer_dev_fatal=Undefined 0\nDLP 0\nSDES 0\nTLP 0\nFCP 0\nCmpltTO 0\nCmpltAbrt 0\nUnxCmplt 0\nRxOF 0\nMalfTLP 0\nECRC 0\nUnsupReq 0\nACSViol 0\nUncorrIntErr 0\nBlockedTLP 0\nAtomicOpBlocked 0\nTLPBlockedErr 0\nPoisonTLPBlocked 0\nTOTAL_ERR_FATAL 0
A: aer_dev_nonfatal=Undefined 0\nDLP 0\nSDES 0\nTLP 0\nFCP 0\nCmpltTO 0\nCmpltAbrt 0\nUnxCmplt 0\nRxOF 0\nMalfTLP 0\nECRC 0\nUnsupReq 0\nACSViol 0\nUncorrIntErr 0\nBlockedTLP 0\nAtomicOpBlocked 0\nTLPBlockedErr 0\nPoisonTLPBlocked 0\nTOTAL_ERR_NONFATAL 0
A: ari_enabled=0
A: broken_parity_status=0
A: class=0x0c0330
H: [encoded data, 8199 characters]
A: consistent_dma_mask_bits=64
A: current_link_speed=5.0 GT/s PCIe
A: current_link_width=1
A: d3cold_allowed=1
A: device=0x8241
A: dma_mask_bits=64
L: driver=../../../../bus/pci/drivers/xhci_hcd
A: driver_override=(null)
A: enable=1
A: irq=16
A: link/clkpm=0
A: link/l0s_aspm=0
A: link/l1_aspm=1
A: local_cpulist=0-3
A: local_cpus=f
A: max_link_speed=5.0 GT/s PCIe
A: max_link_width=1
A: modalias=pci:v0000104Cd00008241sv00001028sd0000050Fbc0Csc03i30
A: msi_bus=1
A: msi_irqs/25=msix
A: msi_irqs/26=msix
A: msi_irqs/27=msix
A: msi_irqs/28=msix
A: msi_irqs/29=msix
A: numa_node=-1
A: pools=poolinfo - 0.1\nbuffer-2048         0    0 2048  0\nbuffer-512          0    0  512  0\nbuffer-128          0    0  128  0\nbuffer-32           0    0   32  0\nxHCI 1KB stream ctx arrays    0    0 1024  0\nxHCI 256 byte stream ctx arrays    0    0  256  0\nxHCI input/output contexts   11   12 2112 12\nxHCI ring segments   34   34 4096 34\nbuffer-2048        16   32 2048 16\nbuffer-512          0    0  512  0\nbuffer-128         26   32  128  1\nbuffer-32           0    0   32  0
A: power/async=enabled
A: power/control=on
A: power/runtime_active_kids=1
A: power/runtime_active_time=6193932
A: power/runtime_enabled=forbidden
A: power/runtime_status=active
A: power/runtime_suspended_time=0
A: power/runtime_usage=1
A: power/wakeup=enabled
A: power/wakeup_abort_count=0
A: power/wakeup_active=0
A: power/wakeup_active_count=0
A: power/wakeup_count=0
A: power/wakeup_expire_count=0
A: power/wakeup_last_time_ms=0
A: power/wakeup_max_time_ms=0
A: power/wakeup_total_time_ms=0
A: power_state=D0
A: reset_method=bus
A: resource=0x00000000f7d00000 0x00000000f7d0ffff 0x0000000000140204\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x00000000f7d10000 0x00000000f7d11fff 0x0000000000140204\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000
A: revision=0x02
A: subsystem_device=0x050f
A: subsystem_vendor=0x1028
A: vendor=0x104c

P: /devices/pci0000:00/0000:00:1c.4
E: DRIVER=pcieport
E: PCI_CLASS=60400
E: PCI_ID=8086:1C18
E: PCI_SUBSYS_ID=1028:050F
E: PCI_SLOT_NAME=0000:00:1c.4
E: MODALIAS=pci:v00008086d00001C18sv00001028sd0000050Fbc06sc04i00
E: SUBSYSTEM=pci
E: ID_PCI_CLASS_FROM_DATABASE=Bridge
E: ID_PCI_SUBCLASS_FROM_DATABASE=PCI bridge
E: ID_PCI_INTERFACE_FROM_DATABASE=Normal decode
E: ID_VENDOR_FROM_DATABASE=Intel Corporation
E: ID_MODEL_FROM_DATABASE=6 Series/C200 Series Chipset Family PCI Express Root Port 5
A: ari_enabled=0
A: broken_parity_status=0
A: class=0x060400
H: [encoded data, 8199 characters]
A: consistent_dma_mask_bits=32
A: current_link_speed=5.0 GT/s PCIe
A: current_link_width=1
A: d3cold_allowed=1
A: device=0x1c18
A: dma_mask_bits=32
L: driver=../../../bus/pci/drivers/pcieport
A: driver_override=(null)
A: enable=2
A: irq=16
A: local_cpulist=0-3
A: local_cpus=f
A: max_link_speed=5.0 GT/s PCIe
A: max_link_width=1
A: modalias=pci:v00008086d00001C18sv00001028sd0000050Fbc06sc04i00
A: msi_bus=1
A: numa_node=-1
A: power/async=enabled
A: power/control=on
A: power/runtime_active_kids=1
A: power/runtime_active_time=6193944
A: power/runtime_enabled=forbidden
A: power/runtime_status=active
A: power/runtime_suspended_time=0
A: power/runtime_usage=2
A: power/wakeup=disabled
A: power/wakeup_abort_count=
A: power/wakeup_active=
A: power/wakeup_active_count=
A: power/wakeup_count=
A: power/wakeup_expire_count=
A: power/wakeup_last_time_ms=
A: power/wakeup_max_time_ms=
A: power/wakeup_total_time_ms=
A: power_state=D0
A: reset_method=pm
A: resource=0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x00000000f7d00000 0x00000000f7dfffff 0x0000000000000200\n0x0000000000000000 0x0000000000000000 0x0000000000000000\n0x0000000000000000 0x0000000000000000 0x0000000000000000
A: revision=0xb5
A: secondary_bus_number=11
A: subordinate_bus_number=12
A: subsystem_device=0x050f
A: subsystem_vendor=0x1028
A: vendor=0x8086

